{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["附件3"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"附件3","index":0,"n_rows":12,"n_cols":13,"rows_kept":12,"merged":[[0,0,0,11],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,12,3,12],[4,0,6,0],[4,1,6,1],[4,2,6,2],[4,3,6,3],[4,4,6,4],[4,5,6,5],[4,12,6,12],[7,0,9,0],[7,1,9,1],[7,2,9,2],[7,3,9,3],[7,4,9,4],[7,5,9,5],[7,12,9,12],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,12,11,13]]}
["附件2：                惠州市2021年6月重点排污企业（废气重点）监督性监测结果（4家）"]
["序号","行政区","企业名称","监测点名称","执行标准名称","监测日期","监测项目名称（单位：mg/m3）","实测浓度","标准限值","是否达标","超标倍数","未监测原因"]
[1,"惠阳区","恒昌涂料（惠阳）有限公司","废气排放口FQ-HY18786","国家标准《涂料、油墨及胶粘剂工业大气污染物排放标准》（GB 37824-2019），苯执行表1中大气污染物排放限值、非甲烷总烃执行表2中大气污染物排放限值","2021-05-27","苯",0.08,1,"是","—","","6月公布            惠阳监测站"]
[{"$nulls":6},"非甲烷总烃",6.01,60,"是","—",""]
[2,"惠阳区","广东艺都科技有限公司","废气排放口","广东省地方标准《印刷行业挥发性有机化合物排放标准》（DB44/815-2010）表2平板印刷第Ⅱ时段有组织排放监控浓度限值","2021-06-08","苯",0.026,1,"是","—","","6月公布            惠阳监测站"]
[{"$nulls":6},"甲苯与二甲苯合计",0.492,15,"是","—",""]
[{"$nulls":6},"总VOCs",0.908,80,"是","—",""]
[3,"惠阳区","胜宏科技（惠州）股份有限公司","废气（涂布车间）排放口DA039","广东省地方标准《印刷行业挥发性有机化合物排放标准》（DB44/815-2010）丝网印刷第Ⅱ时段有组织排放监控浓度限值","2021-06-25","苯",0.053,1,"是","—","","6月公布            惠阳监测站"]
[{"$nulls":6},"甲苯与二甲苯合计",0.164,15,"是","—",""]
[{"$nulls":6},"总VOCs",0.462,120,"是","—",""]
[4,"大亚湾经济技术开发","深圳信立泰药业股份有限公司大亚湾制药厂","工艺有机废气排气口DA001","制药工业大气污染物排放标准GB37823—2019,恶臭污染物排放标准GB 14554-93,大气污染物排放限值DB44/ 27—2001,锅炉大气污染物排放标准DB44/765-2019","2021-06-01","丙酮",6.38,320,"是","—",null,"6月公布            大亚湾监测站"]
[{"$nulls":6},"乙酸乙酯",2.83,40,"是","—"]