{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地下水"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地下水","index":0,"n_rows":15,"n_cols":25,"rows_kept":15,"merged":[[0,0,0,24],[1,6,1,24],[3,0,6,0],[3,1,6,1],[7,0,7,2],[9,0,13,0]],"flags":["formulas_cached_only"]}
["附件3：                         惠州市2022年3月生活垃圾处理企业地下水监测结果（3家）"]
[{"$nulls":6},"单位：毫克/升（除PH值无量纲，粪大肠菌群为个/升外）"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅","粪大肠菌群"]
["惠东县垃圾填埋场","2022-02-11","废水站1号监测井",5.76,67.8,215,11.2,43.3,0.543,{"v":0.87,"d":"0.870"},0.00048,0.00908,"0.0003L",0.7,1.93,0.008,0.27,0.129,"0.001L","0.00004L","0.0003L",0.00035,"0.004L",0.00322,"20L"]
[null,null,"评价","偏低0.74个pH","达标","达标","达标","达标","超0.81倍","超7.70倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
[null,null,"项目正北方向3号扩散井",5.12,131,526,1.07,260,0.514,0.305,0.00262,0.257,"0.0003L",1.3,0.438,"0.003L",0.15,0.134,"0.001L","0.00004L",{"v":0.001,"d":"0.0010"},0.00367,"0.004L",0.00206,"20L"]
[null,null,"评价","偏低1.38个pH","达标","达标","达标","超0.04倍","超0.71倍","超2.05倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
["《地下水质量标准》（GB/T14848-2017）Ⅲ类",null,null,"6.5—8.5",450,1000,250,250,0.3,0.1,{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},0.002,3,20,{"v":1,"d":"1.00"},{"v":0.5,"d":"0.50"},{"v":1,"d":"1.0"},0.05,0.001,0.01,0.005,0.05,0.01,"—"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅","粪大肠菌群"]
["惠阳区榄子垅垃圾综合处理项目生活垃圾填埋场","2022-02-10","1#地下水井取样点",6.41,24.1,126,1.94,17.9,1.04,0.565,0.00524,0.0275,"0.0003L",1.2,0.306,0.007,0.18,0.882,"0.001L","0.00004L",0.0009,6e-05,"0.004L",0.00257,1100]
[null,"2022-02-10","2#地下水井取样点",5.98,176,909,45.9,265,0.0459,0.00664,0.00379,0.0645,"0.0003L",1.9,1.78,"0.003L",0.15,1.84,"0.001L","0.00004L",0.0003,0.00085,"0.004L",0.00066,"20L"]
[null,"2022-02-10","3#地下水井取样点",5.86,2.14,26,1.05,7.64,0.0533,0.0232,0.00342,0.0189,"0.0003L","0.5L",0.421,"0.003L",{"v":0.1,"d":"0.10"},0.053,"0.001L","0.00004L",0.0008,0.00042,"0.004L",{"v":0.0049,"d":"0.00490"},"20L"]
[null,"2022-02-10","4#地下水井取样点",5.16,314,"1.31×103",21.1,{"v":38,"d":"38.0"},7.65,1.27,0.00339,0.0296,"0.0003L",3.9,0.593,0.006,5.56,0.154,"0.001L","0.00004L",0.0003,6e-05,"0.004L",0.00176,"20L"]
[null,"2022-02-10","6#地下水井取样点",{"v":5.9,"d":"5.90"},26.1,131,{"v":4.5,"d":"4.50"},31.7,26.5,22.3,0.00916,1.95,"0.0003L",1.9,0.318,"0.003L",0.35,1.31,"0.001L","0.00004L",0.0004,0.00472,"0.004L",0.0554,"20L"]
["龙门县垃圾填埋场\n（龙门县甘香垃圾场）","2022-02-24","垃圾场地下水监测井",5.23,21.3,134,11.2,40.7,0.558,{"v":0.12,"d":"0.120"},0.00241,0.137,"0.0003L",1.8,1.35,"0.003L",{"v":0.2,"d":"0.20"},0.095,"0.001L","0.00004L","0.0003L",0.00014,"0.004L",0.00299,40]