{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["舞台灯光音响"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"舞台灯光音响","index":0,"n_rows":105,"n_cols":8,"rows_kept":105,"merged":[[0,0,0,7],[1,0,1,7],[3,0,41,0],[3,1,3,7],[4,1,4,7],[9,1,9,7],[17,1,17,7],[25,1,25,7],[26,1,26,7],[35,1,35,7],[39,1,39,7],[42,0,42,7],[43,0,43,7],[44,3,44,4],[45,0,63,0],[45,1,56,1],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,3,50,4],[51,3,51,4],[52,3,52,4],[53,3,53,4],[54,3,54,4],[55,3,55,4],[56,3,56,4],[57,1,63,1],[57,3,57,4],[58,3,58,4],[59,3,59,4],[60,3,60,4],[61,3,61,4],[62,3,62,4],[63,3,63,4],[64,0,64,7],[65,0,65,7],[66,3,66,4],[67,0,73,0],[67,1,68,1],[67,2,68,2],[67,3,68,4],[69,3,69,4],[70,3,70,4],[71,3,71,4],[72,3,72,4],[73,3,73,4],[74,0,74,7],[75,0,75,7],[76,0,90,0],[76,3,76,4],[77,3,77,4],[78,3,78,4],[79,3,79,4],[80,3,80,4],[81,3,81,4],[82,3,82,4],[83,3,83,4],[84,3,84,4],[85,3,85,4],[86,3,86,4],[87,3,87,4],[88,3,88,4],[89,3,89,4],[90,3,90,4],[91,0,91,7],[92,0,92,7],[93,3,93,4],[94,0,104,0],[94,1,104,1],[94,2,104,2],[94,3,94,4],[95,3,95,4],[96,3,96,4],[97,3,97,4],[98,3,98,4],[99,3,99,4],[100,3,100,4],[101,3,101,4],[102,3,102,4],[103,3,103,4],[104,3,104,4]],"flags":["formulas_cached_only"]}
["惠州文化艺术中心设备设施更换维修项目清单"]
["舞台灯光、音响维保服务项目"]
["项目","序号","设备名称","项目特征/内容","品牌","规格型号","单位","数量"]
["舞台设备检修","一、舞台灯光系统"]
[null,"（一）灯光控台升级"]
[null,1,"电脑灯光控制台","升级新版本，检查维护","MA3","grandMA3 light","项",1]
[null,2,"电脑灯光控制台","升级新版本，检查维护","MA3","grandMA3 compact ","项",1]
[null,3,"电脑灯光控制台","升级新版本，检查维护","MA3","MA3wing","项",1]
[null,4,"灯光控制台","升级新版本，检查维护","FlyingPig","Road Hog","项",1]
[null,"（二）灯光系统设备软件、硬件检修"]
[null,1,"字幕系统","各类接口接线检查、紧固，系统稳定性检查及测试，拆机除尘维护。","灵星雨","P3室内全彩显示屏：三组 P3(1R1B1G)","项",1]
[null,2,"灯光控制系统","各控制台的输出/输入接口的检查，运行的可靠性、稳定性检查。","Strand 斯全德 ",null,"项",1]
[null,3,"灯光网络系统","输入/输出接口的检查,重点测试导通及极性状态。","Strand 斯全德 ",null,"项",1]
[null,4,"调光硅柜、直通柜","调光硅柜可靠性、稳定性检查，各接口的检查与紧固，拆机除尘维护。","Strand 斯全德 ","CD80-XP\n共1152回路","套",12]
[null,5," 场灯调光硅","调光硅柜可靠性、稳定性检查，各接口的检查与紧固，拆机除尘维护。","Strand 斯全德","共120回路（12路调光）×6KW ","套",10]
[null,6,"信号处理柜（灯光控制室）（监督位）（硅柜室）","交换机、转换器、放大器。可靠性、稳定性检查，各接口的检查与紧固，拆机除尘维护。","华为/Strand 斯全德","Ethernet交换机、Ethernet/DMX转换器、放大器。 ","项",3]
[null,7,"舞台灯具及舞台效果设备","各接口的检查与紧固，更换老化线路、接插件及配件，拆机除尘维护。","AntariHZ500NovaCorpEH-6.0 ","烟机、雪花机、干冰机、泡泡机\n\n\n","项",1]
[null,"（三）灯光系统接口、线路检修、绝缘检测"]
[null,1,"（一道）面光灯","各接口的检查与紧固，更换老化线路、接插件及配件，拆机除尘维护。","ETC","Source Four 5°","台",30]
[null,2,"（二道）面光灯","各接口的检查与紧固，更换老化线路、接插件及配件，拆机除尘维护。","ETC","Source Four 10°","台",30]
[null,3,"电脑灯","各接口的检查与紧固，更换老化线路、接插件及配件，拆机除尘维护。","FINE ","1800BSWF/EWF","台",60]
[null,4,"舞台帕灯","各接口的检查与紧固，更换老化线路、接插件及配件，拆机除尘维护。","ETC","575par","只",70]
[null,5,"DMX信号插座检修","各接口的检查与紧固补焊，更换老化线路、配件，拆机除尘维护。","Strand 斯全德 ",null,"项",1]
[null,6,"直通电源插座检修","各接口的检查与紧固，更换老化线路、配件。",null,null,"项",1]
[null,7,"调光电源插座检修","各接口的检查与紧固，更换老化线路、配件，除尘维护",null,null,"项",1]
[null,"二、舞台音响系统"]
[null,"（一）音响系统设备软件、硬件检修"]
[null,1,"扬声器系统","扬声器接线检查、紧固，稳定性检查及测试，吊挂件螺栓的检查与紧固，拆机除尘维护。","EAW","KF850","台",38]
[null,2,"数字调音台系统","控制界面、路由器、DSP处理器、输入/输出机站、的连接、控制检查，系统运行的可靠性、稳定性检查，拆机除尘维护。","VENUE","Digidesign-Show","项",1]
[null,3,"模拟调音台系统","按键、旋钮、推子、指示灯的功能检查，输入/输出通道的接插件检查，拆机除尘维护。","ALLEN&HE ","ATHML4800-48","项",1]
[null,4,"音频周边设备","功能键及输入输出通道检查","YAMAHA"," DWE64NT\\C electronic M300","项",1]
[null,5,"功率放大器系统","操作界面、预置程序及功能键的检查，输入/输出通道及对应接插件检查。","Powersoft","Q4004R 系列","项",1]
[null,6,"音频处理器","操作界面、预置程序及功能键的检查，输入/输出通道及对应接插件检查。","YAMAHA","DME64N","项",1]
[null,7,"音频分配器","操作界面、预置程序及功能键的检查，输入/输出通道及对应接插件检查。","KLARK-TEKNIK ","DN1248+","项",1]
[null,8,"无线及有线话筒","按键及性能检查，信号输入输出的检查。","SHURE ","UR4D+/KSM9","项",1]
[null,"（二）音响系统线路及接口检修"]
[null,1,"跳线盘检修","跳线接口的检查，焊接线路的检查补焊。",null,null,"项",1]
[null,2,"音频信号插座检修","各接口的检查与紧固补焊，更换老化线路、配件。",null,null,"项",1]
[null,3,"视频及电源线路检修","各接口的检查与紧固补焊，更换老化线路、配件。",null,null,"项",1]
[null,"（三）数字调音台系统软件升级"]
[null,1,"数字调音台","升级新版本，检查维护","VENUE","Digidesign","项",1]
[null,2,"音响声场测试","进行最大声压级、声场不均匀度、传声增益、传输频率特性测试，并调试至最佳使用效果","各演出厅",null,"项",1]
[]
["舞台设备更换"]
["项目","序号","设备名称","项目参数要求",null,"规格型号","单位","数量"]
["LED显示屏设备增购",1,"LED显示屏","屏体尺寸：6.042m*1.05m; 像数点间距 3mm 像素密度 111111 Dots/㎡\n像素构成 1R1G1B 灯管封装 SMD2020\n尺寸(长*宽*厚) 192*192*15mm 重量 0.23kg±0.01kg\n结构特点 软连接 模组分辨率 64*64=4096 dots\n输入电压(直流) 4.2~5V（典型 4.5V） 最大电流 ≤3.2A\n信号输入接口类型 HUB75（两组数据） 级联 可级联\n模组功率 ≤15W 驱动方式 恒流驱动\n40A 电源带模组数 ≤8 张 60A 电源带模组数 ≤12 张\n亮度 600cd/㎡（典型值） 亮度均匀性 ＞0.95\n屏幕水平视角 160±10 度 屏幕垂直视角 140±10 度\n最佳视距 ≥7m 使用环境 室内\n使用寿命 ≥10 万小时 平均无故障时间 ≥5000 小时\n衰减率(工作 3 年) ≤10％ 连续失控点 0\n离散失控点 ＜30PPM，出厂时为 0 盲点率 ＜50PPM，出厂时为 0\n工作温度范围 -10℃~40℃ 工作湿度范围 10％~65％RH(无结露)\n模组平整度 ＜0.2mm 刷新 1920~3840Hz（根据需求）\n色温 2000K~14000K（可调） 对比度 3000:1\n备注*为了延长使用寿命,建议配置负载时多留30%的余量。例如:设备需要100W的",null,"P3","平方",6.3441]
[null,null,"屏幕电源/辅材","电流范围 0～40A，额定功率 180W，纹波与噪声 150mVp-p\n电压调节范围 ±5%，电压精度 ±1.0%，线性调整率 ±0.5%，负载调整率 ±2%\n启动、上升时间 2000ms，50ms/230VAC 负载100%\n保持时间（Typ） 20ms/230VAC 负载100%\n输入电压范围 200～240VAC，频率范围 47～63HZ，功率因数 （Typ） PF≥0.5，效率（Typ） ≥86% ≥87%\n交流电流 115VAC / /，230VAC 2.5A 2.5A，浪涌电流（Typ）60A/230VAC，泄漏电流 <1mA/230VAC\n保护过负载 110～150% rated，短路 输出端短路后电源保护，消除短路后可自动恢复输出\n过电压 /过温度 /\n环境：工作温度 -20℃～+50℃ (AC 230V)(参考负载温度降额曲线)，工作湿度 20～90%RH不凝固，储存温度 -30～+85℃，储存湿度 10～95%RH 不凝固，温度系数 ±0.03%/℃（0～50℃）\n耐振动 10～500Hz，2G，10min/周期，X、Y、Z方向各60min\n安全规定 设计参考GB4943-2001，UL1012\n耐压 I/P-O/P：3.0KVAC I/P-FG：1.5KVAC O/P-FG：0.5KVAC\n绝缘阻抗 I/P-O/P、I/P-FG、O/P-FG：大于50MΩ/500VDC/25℃/70%RH\nEMC 设计参考GB9254 EN55022，Class B\n谐波电流 设计参考GB17625.1;EN61000-3-2,-3 限值要求\n电磁耐受 设计参考EN55024 ;EN61000-4-2,3,4,5,6,8,11\n其它 寿命 100,000小时(25℃)，尺寸 190*82*30mm（长*宽*高），包装 0.40Kg/只\n备注*为了延长使用寿命,建议配置负载时多留30%的余量。例如:设备需要100W的",null,"直流电源4.5V\n额定电流 40A\n","项",1]
[null,null,"接收卡","含软件：支持16组和32组数据输出模式；\n单卡自带16个HUB75  16P接口；\n单卡带载像素128*1024/256*512。\n支持逐点亮色度校正、多批次、亮暗线调节和显示屏效果调节等功能，与3D控制器搭配支持3D效果；\n支持接收卡预存画面和保留最后一帧设置；\n支持灯板flash管理；\n支持5pin液晶模块；\n支持千兆网，可通过网线直接连接PC端进行调试和显示；\n支持接收卡参数及程序包回读；\n接收卡具有与灯板一致的电源接口；",null,"LED显示屏接收系统V1.0单卡","项",1]
[null,null,"视频处理器","输入：1*DVI，1*HDMI1.3，1*VGA，1*USB  播  放，1*CVBS；\n输出：4 路网口输出，带载 260万，最宽3840，最高 1920，单画面显示",null,"V960","套",1]
[null,null,"笔记本","联想r7000p",null,null,"台",1]
[null,null,"控制软件",{"$nulls":3},"套",1]
[null,null,"框架结构","根据现场定制落地式安装",null,null,"平方",6.7]
[null,null,"弱电线缆","3根网线，根据现场实际情况结算或客户自备"]
[null,null,"强电电缆","根据现场实际情况结算或客户自备"]
[null,null,"配电箱","配电箱配电箱",null,"10kw","套",1]
[null,null,"控制主机","I5；16G内存；120G固态；20寸显示器；无线键鼠套装,",null,null,"套",1]
[null,null,"施工费","施工、设备、运输、安装、调试特殊环境另行协商",null,null,"平方 ",6.3]
[null,2,"LED显示屏","1.产品型号：RP3.9\n2.像素间距 (mm)：3.91\n3.LED类型：SMD2020\n4.像素组成：1R1G1B\n5.箱体尺寸 (mm)：500x500x73.5\n6.箱体分辨率 (pixels)：128X128\n7.模组尺寸 (mm)：250x250x15.8\n8.模组分辨率 (pixels)：64X64\n9.最大白平衡亮度(NIT)：700\n10.重量 (kg)：13\n11.对比度：≥3000:1\n12.主结构材质：压铸铝\n13.灰度等级 (BIT)：13-14\n14.刷新频率 (Hz)：3840\n15.视角（水平 /垂直）：140°/120°\n16.功耗（最大/平均W/㎡）：500/170\n17.工作温度：-10℃～ 40℃\n18.工作湿度：10%RH～ 60%RH（无凝露）",null,"P3.91","平方",17.5]
[null,null,"笔记本","联想r7000p",null,null,"台",2]
[null,null,"航空箱","500*500箱体，一拖八。",null,null,"平方",17.5]
[null,null,"日子架","可拆卸，任意组装",null,null,"平方",17.5]
[null,null,"视频处理器","输入：1*DVI，1*HDMI1.3，1*VGA，1*USB  播  放，1*CVBS；\n输出：4 路网口输出，带载 260万，最宽3840，最高 1920，单画面显示",null,"V960","套",1]
[null,null,"配电箱","标准配电箱",null,"20kw","套",1]
[null,null,"备品","同批",null,null,"平方",1]
[]
["设备设施更换"]
["项目","序号","设备名称","项目参数要求",null,"    规格型号","单位","数量"]
["储物柜更换",1,"人脸识别管理系统","终端系统:可实现人员、终端的基础信息管理、人员和用户权限管理、管理日志及报表生成、柜子使用情况、故障设置、远程开门等功能，固定或大众模式，支持二次开发",null,"36门","套",3]
[{"$nulls":5},"48门","套",1]
[null,2,"智能储物柜","安装方式：插电即用\n柜体材质：优质电解板，厚度不少于0.8mm，符合环保要求。其中格内径：宽度>=327mm，高度>=284mm，深度>=450mm柜体带应急锁，\n可串联10台副柜以上。不易被破坏。带触摸屏幕和双目人脸识别。\n电源：220V ±10%，50/60HZ，功率150W内\n工作环境：工作温度-20摄氏度至60摄氏度，适应湿度在20%RH到90%RH（无凝露）\n",null,"柜体尺寸:宽度850mm，高度1800mm，深度460mm（正负差距在1mm以内）","台",13]
[null,3,"人脸识别","（1）最大用户数:≥10000个人脸模板；（2）识别速度: <=1s;\n（3）识别率: >=99%;\n（4）误识率: <=0.1%;\n（5）角度范围: 水平：±20°, 垂直：±20\n（6）误识率: <=0.1%;\n（7）人体自动感应：支持；\n认假率<0.001%,拒真率<0.1%。支持1：1和1：N比对模式，预留指纹识别等其它识别方式端口\n",null,"人脸模板","台",4]
[null,4,"触摸式显示屏","柜体集成不小于7寸工控触摸屏（带语音提示功能），支持window、安卓或linux等操作系统。",null,"7寸工控触摸屏","台",4]
[null,5,"工控板","主控系统至少双核四线程以上，主频至少1GHZ。供应商需提供详细的工控板参数。",null,null,"台",4]
[null,6,"其他","含音箱、电源、线材、锁扣、运输安装及调试实施。",{"$nulls":3},1]
[]
["防爆器材更换"]
["防爆器材更换","序号","设备名称","项目参数要求",null,"规格型号","单位","数量"]
[null,1,"防暴器材柜","高180cm*宽90cm*深55cm",null,"加厚钢材/环保喷漆","个",2]
[null,2,"防暴器材置物架","110cm*40cm*115cm",null,"3C钢化玻璃","个",1]
[null,3,"防暴盾牌","90cm*50cm",null,"PC/5.0MM","套",4]
[null,4,"防暴钢叉","收缩约130cm伸长约210cm*45cm",null,"钢","个",4]
[null,5,"防割手套",null,null,"涤纶丝、钢丝","副",4]
[null,6,"防暴脚叉","收缩约130cm伸长约195cm*28cm",null,"不锈钢","套",4]
[null,7,"防暴头盔","28.5cm*15cm*25cm",null,"钢盔","个",4]
[null,8,"防刺服","约1.85KG",null,"高性能纤维材料","副",4]
[null,9,"防暴棍","50cm",null,"PC","个",4]
[null,10,"强光手电","长18CM、350流明及以上",null,"铝合钢","个",15]
[null,11,"安保腰带","125cm*5cm",null,"帆布、合金","条",6]
[null,12,"伸缩警棍","收回24cm展开65cm",null,"合金钢","根",6]
[null,13,"辣椒水","60ml",null,null,"瓶",10]
[null,14,"隔离带","2米带长黑杆，高度90米，底座直径32厘米",null,"铁烤漆","套",50]
[]
["工程设备维修"]
["项目","序号","设备名称","项目参数要求",null,"规格型号","单位","数量"]
["空调维修",1,"控制室空调","美的压缩机",null,"同型号设备","台",1]
[{"$nulls":3},"美的多联机主板维修",null,"同型号设备","台",1]
[{"$nulls":3},"主机电路维修",null,"同型号设备","台",1]
[{"$nulls":3},"室内机控制主板更换",null,"同型号设备","块",1]
[{"$nulls":3},"美的多联机控制器",null,"同型号设备","个",4]
[{"$nulls":3},"雪种R22",null,"同型号设备","KG",13]
[{"$nulls":3},"室内天花机清洗保养",null,null,"台",4]
[{"$nulls":3},"美的多联机主机清洗保养",null,null,"台",2]
[{"$nulls":3},"五金辅助材料",null,"同型号设备","项",1]
[{"$nulls":3},"文明施工规费",null,null,"项",1]
[{"$nulls":3},"垃圾清理",null,null,"项",1]