{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["附件1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"附件1","index":0,"n_rows":283,"n_cols":10,"rows_kept":283,"merged":[[0,0,0,9],[2,0,10,0],[2,1,10,1],[2,2,10,2],[2,3,7,3],[2,4,10,4],[2,5,10,5],[8,3,9,3],[11,0,25,0],[11,1,25,1],[11,2,25,2],[11,3,22,3],[11,4,25,4],[11,5,25,5],[23,3,24,3],[26,0,34,0],[26,1,34,1],[26,2,34,2],[26,3,31,3],[26,4,34,4],[26,5,34,5],[32,3,33,3],[35,0,42,0],[35,1,42,1],[35,2,42,2],[35,3,42,3],[35,4,42,4],[35,5,42,5],[43,0,45,0],[43,1,45,1],[43,2,45,2],[43,3,45,3],[43,4,45,4],[43,5,45,5],[46,0,52,0],[46,1,52,1],[46,2,52,2],[46,3,52,3],[46,4,52,4],[46,5,52,5],[53,0,54,0],[53,1,54,1],[53,2,54,2],[53,3,54,3],[53,4,54,4],[53,5,54,5],[55,0,61,0],[55,1,61,1],[55,2,61,2],[55,3,61,3],[55,4,61,4],[55,5,61,5],[62,0,67,0],[62,1,67,1],[62,2,67,2],[62,3,67,3],[62,4,67,4],[62,5,67,5],[68,0,73,0],[68,1,73,1],[68,2,73,2],[68,3,73,3],[68,4,73,4],[68,5,73,5],[74,0,81,0],[74,1,81,1],[74,2,81,2],[74,3,81,3],[74,4,81,4],[74,5,81,5],[82,0,86,0],[82,1,86,1],[82,2,86,2],[82,3,86,3],[82,4,86,4],[82,5,86,5],[87,0,96,0],[87,1,96,1],[87,2,96,2],[87,3,96,3],[87,4,96,4],[87,5,96,5],[97,0,100,0],[97,1,100,1],[97,2,100,2],[97,3,100,3],[97,4,100,4],[97,5,100,5],[101,0,108,0],[101,1,108,1],[101,2,108,2],[101,3,108,3],[101,4,108,4],[101,5,108,5],[109,0,113,0],[109,1,113,1],[109,2,113,2],[109,3,113,3],[109,4,113,4],[109,5,113,5],[114,0,118,0],[114,1,118,1],[114,2,118,2],[114,3,118,3],[114,4,118,4],[114,5,118,5],[119,0,127,0],[119,1,127,1],[119,2,127,2],[119,3,124,3],[119,4,127,4],[119,5,127,5],[125,3,126,3],[128,0,141,0],[128,1,141,1],[128,2,141,2],[128,3,138,3],[128,4,141,4],[128,5,141,5],[139,3,140,3],[142,0,146,0],[142,1,146,1],[142,2,146,2],[142,3,146,3],[142,4,146,4],[142,5,146,5],[147,0,156,0],[147,1,156,1],[147,2,156,2],[147,3,156,3],[147,4,156,4],[147,5,156,5],[157,0,161,0],[157,1,161,1],[157,2,161,2],[157,3,161,3],[157,4,161,4],[157,5,161,5],[162,0,165,0],[162,1,165,1],[162,2,165,2],[162,3,165,3],[162,4,165,4],[162,5,165,5],[166,0,172,0],[166,1,172,1],[166,2,172,2],[166,3,172,3],[166,4,172,4],[166,5,172,5],[173,0,177,0],[173,1,177,1],[173,2,177,2],[173,3,177,3],[173,4,177,4],[173,5,177,5],[178,0,186,0],[178,1,186,1],[178,2,186,2],[178,3,186,3],[178,4,186,4],[178,5,186,5],[187,0,193,0],[187,1,193,1],[187,2,193,2],[187,3,192,3],[187,4,192,4],[187,5,193,5],[194,0,198,0],[194,1,198,1],[194,2,198,2],[194,3,198,3],[194,4,198,4],[194,5,198,5],[199,0,207,0],[199,1,207,1],[199,2,207,2],[199,3,207,3],[199,4,207,4],[199,5,207,5],[208,0,215,0],[208,1,215,1],[208,2,215,2],[208,3,214,3],[208,4,215,4],[208,5,215,5],[216,0,226,0],[216,1,226,1],[216,2,226,2],[216,3,225,3],[216,4,226,4],[216,5,226,5],[227,0,232,0],[227,1,232,1],[227,2,232,2],[227,3,232,3],[227,4,232,4],[227,5,232,5],[233,0,238,0],[233,1,238,1],[233,2,238,2],[233,3,238,3],[233,4,238,4],[233,5,238,5],[239,0,248,0],[239,1,248,1],[239,2,248,2],[239,3,248,3],[239,4,248,4],[239,5,248,5],[249,0,253,0],[249,1,253,1],[249,2,253,2],[249,3,253,3],[249,4,253,4],[249,5,253,5],[254,0,260,0],[254,1,260,1],[254,2,260,2],[254,3,260,3],[254,4,260,4],[254,5,260,5],[261,0,266,0],[261,1,266,1],[261,2,266,2],[261,3,265,3],[261,4,266,4],[261,5,266,5],[267,0,277,0],[267,1,277,1],[267,2,277,2],[267,3,276,3],[267,4,277,4],[267,5,277,5],[278,0,282,0],[278,1,282,1],[278,2,282,2],[278,3,282,3],[278,4,282,4],[278,5,282,5]]}
["附件1：         惠州市2025年1-12月重点排污企业（废水重点）监督性监测结果（监测站）"]
["序号","行政区","企业名称","监测点名称","执行标准名称","监测日期","监测项目名称       （单位：mg/L）","污染物浓度","标准限值","是否达标"]
[1,"仲恺区","惠阳钰原工业有限公司","综合废水排放口DW003","广东省地方标准《电镀水污染物排放标准DB/441597-2015》表1现有项目谁污染物排放限值及单位产品基准排水量珠三角排放限值","2025-01-08","总磷",0.02,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"氨氮",{"v":0.15,"d":"0.150"},10,"是"]
[{"$nulls":6},"化学需氧量",7,80,"是"]
[{"$nulls":6},"总氮",3.38,20,"是"]
[{"$nulls":6},"总氯化物",0.018,0.2,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":3},"含铬废水排放口DW002",null,null,"总铬",0.05,0.5,"是"]
[{"$nulls":6},"六价铬","ND",0.1,"是"]
[{"$nulls":3},"含镍废水排放口DW001",null,null,"总镍","ND",0.5,"是"]
[null,"仲恺区","惠阳钰原工业有限公司","废水排放口DW003","执行《电镀水污染物排放限值》（DB44/1597-2015)表1现有项目水污染物排放限值及单位产品基准排水量珠三角排放限值和《水污染物排放限值》DB44/26-2001表2第二类污染物最高允许排放浓度（第一时段）一级标准限值两者之中的较严值。","2025-10-24","悬浮物","ND",30,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"总磷",0.02,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"总氮",2.72,20,"是"]
[{"$nulls":6},"化学需氧量",21,80,"是"]
[{"$nulls":6},"氟化物",0.33,10,"是"]
[{"$nulls":6},"石油类",0.07,2,"是"]
[{"$nulls":6},"总氰化物",{"v":0.01,"d":"0.010"},0.2,"是"]
[{"$nulls":6},"总铁","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":6},"总锌","ND",{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"pH值",7.4,"6-9","是"]
[{"$nulls":3},"废水排放口DW002",null,null,"总铬",0.04,0.5,"是"]
[{"$nulls":6},"六价铬","ND",0.1,"是"]
[{"$nulls":3},"废水排放口DW001",null,null,"镍","ND",0.5,"是"]
[2,"仲恺区","惠阳源高电器有限公司","综合废水排放口DW003","广东省地方标准《电镀水污染物排放标准DB/441597-2015》表1现有项目谁污染物排放限值及单位产品基准排水量珠三角排放限值","2025-01-08","总磷",0.04,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"氨氮",0.201,10,"是"]
[{"$nulls":6},"化学需氧量",44,80,"是"]
[{"$nulls":6},"总氮",8.71,20,"是"]
[{"$nulls":6},"总氯化物",0.005,0.2,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":3},"含铬废水排放口DW002",null,null,"总铬",0.04,0.5,"是"]
[{"$nulls":6},"六价铬","ND",0.1,"是"]
[{"$nulls":3},"含镍废水排放口DW001",null,null,"总镍","ND",0.5,"是"]
[3,"仲恺区","中信惠州医院有限公司","废水排放口DW001","执行《医疗机构谁污染物排放标准》（GB18466-2005)中表2综合医疗机构和其他医疗机构谁污染物排放限值（日均值）排放标准，其中氨氮执行《水污染物排放限值》（DB44/26-2001）表4第二类污染物最高允许排放浓度（第二时段）中一级标准排放限值","2025-01-15","总余氯",0.05,0.5,"是"]
[{"$nulls":6},"粪大肠菌群",60,500,"是"]
[{"$nulls":6},"氨氮",0.502,10,"是"]
[{"$nulls":6},"化学需氧量",15,60,"是"]
[{"$nulls":6},"阴离子表面活性剂",0.12,5,"是"]
[{"$nulls":6},"动植物油","ND",5,"是"]
[{"$nulls":6},"总氯化物","ND",0.5,"是"]
[{"$nulls":6},"挥发酚","ND",0.5,"是"]
[4,"仲恺区","广东太古可口可乐惠州有限公司","废水总排口WS-07001","《水污染物排放限值》（DB44/26-2001）表4第二时段二级标准限值","2025-01-06","磷酸盐",0.05,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"氨氮",0.176,15,"是"]
[{"$nulls":6},"化学需氧量",18,110,"是"]
[5,"仲恺区","广东太古可口可乐惠州有限公司","WS-07001废水总排口","《水污染物排放限值》（DB44/26-2001）表4第二时段二级标准限值","2025-07-14","石油类","ND",{"v":8,"d":"8.0"},"是"]
[{"$nulls":6},"氨氮",0.224,15,"是"]
[{"$nulls":6},"化学需氧量",18,110,"是"]
[{"$nulls":6},"磷酸盐",0.87,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"挥发酚",0.14,0.5,"是"]
[{"$nulls":6},"悬浮物","ND",100,"是"]
[{"$nulls":6},"pH值",7.88,"6-9","是"]
[6,"仲恺区","广东伊利乳业有限责任公司","废水排放口DW001","执行《城镇污水处理厂污染物排放标准》（GB18918-2002）表1基本控制项目最高允许排放浓度（日均值）一级标准B标准","2025-02-24","化学需氧量",26,60,"是"]
[{"$nulls":6},"氨氮",3.11,8,"是"]
[7,"仲恺区","广东伊利乳业有限责任公司","WS-07001废水排口","执行《广东省水污染物排放限值》（DB44/26-2001)表4第二类污染物最高允许排放浓度（第二时段）三级标准限值。","2025-07-22","动植物油",0.16,100,"是"]
[{"$nulls":6},"氨氮",0.144,25,"是"]
[{"$nulls":6},"化学需氧量",30,250,"是"]
[{"$nulls":6},"色度",3,"-","是"]
[{"$nulls":6},"悬浮物","ND",300,"是"]
[{"$nulls":6},"五日生化需氧量",8.3,200,"是"]
[{"$nulls":6},"pH值",7.3,"6-9","是"]
[7,"仲恺区","格雷蒙科技（惠州）有限公司","废水排放口DW001","化学需氧量执行《水污染物排放限值》（DB44/26-2001)表4第二类污染物最高允许排放浓度第二时段城镇二级污水处理厂一级标准，其余执行《电镀水污染物排放标准》（DB44/1597-2015)表2新建项目水污染物排放限值及单位产品基准排水量珠三角排放限值标准。","2025-02-24","化学需氧量",14,40,"是"]
[{"$nulls":6},"氨氮",0.816,8,"是"]
[{"$nulls":6},"总磷",0.03,0.5,"是"]
[{"$nulls":6},"总氮",1.68,15,"是"]
[{"$nulls":6},"总铜","ND",0.3,"是"]
[{"$nulls":6},"总锌","ND",{"v":1,"d":"1.0"},"是"]
[null,"仲恺区","格雷蒙科技（惠州）有限公司","废水排放口DW001","执行《电镀水污染物排放标准》DB441597-2015表1现有项目水污染物排放限值及单位产品基准排水量珠三角排放限值200%，执行《电子工业水污染物排放标准》GB39731-2020表1水污染物排放限值间接排放限值。","2025-09-30","悬浮物","ND","60","是"]
[{"$nulls":6},"阴离子表面活性剂","ND","20","是"]
[{"$nulls":6},"石油类","ND","4","是"]
[{"$nulls":6},"氟化物",0.22,"20","是"]
[{"$nulls":6},"硫化物","ND","1","是"]
[{"$nulls":6},"pH值",{"v":8,"d":"8.0"},"6-9","是"]
[8,"仲恺区","惠州市中心人民医院仲恺院区","废水排放口DW001","执行《医疗机构水污染物排放标准》(GB18466-2005)中表2综合医疗机构和其他医疗机构水污染区排放限值（日均值）预处理标准（总余氯1）采用含氧消毒剂消毒的工艺控制要求为：预处理标准：消毒接触池接触时间≥1h，接触池出口总余氯2-8mg/L）","2025-03-03","总余氯1",5.24,"2-8","是"]
[{"$nulls":6},"粪大肠菌群",230,5000,"是"]
[{"$nulls":6},"氨氮",25.5,"/","是"]
[{"$nulls":6},"化学需氧量",34,250,"是"]
[{"$nulls":6},"阴离子表面活性剂",0.06,10,"是"]
[{"$nulls":6},"动植物油","ND",20,"是"]
[{"$nulls":6},"总氯化物",{"v":0.01,"d":"0.010"},0.5,"是"]
[{"$nulls":6},"挥发酚",0.09,{"v":1,"d":"1.0"},"是"]
[9,"仲恺区","惠州市星之光科技有限公司","废水排放口DW001","执行《电镀水污染物排放标准》（DB44/1597-2015)表1的珠三角标准。","2025-03-10","总磷",0.047,{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"氨氮",0.569,30,"是"]
[{"$nulls":6},"化学需氧量",28,160,"是"]
[{"$nulls":6},"总铜",0.26,0.5,"是"]
[{"$nulls":6},"总氮",7.79,40,"是"]
[10,"仲恺区","惠州市星之光科技有限公司","废水排放口DW001","执行《电镀水污染物排放标准》（DB44/1597-2015)表1的珠三角标准。","2025-07-17","总氮",5.61,40,"是"]
[{"$nulls":6},"氨氮",{"v":0.65,"d":"0.650"},30,"是"]
[{"$nulls":6},"总磷",{"v":0.2,"d":"0.20"},{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"化学需氧量",25,160,"是"]
[{"$nulls":6},"氰化物","ND",0.2,"是"]
[{"$nulls":6},"氟化物",0.08,{"v":10,"d":"10.0"},"是"]
[{"$nulls":6},"石油类",0.1,4,"是"]
[{"$nulls":6},"悬浮物","ND",60,"是"]
[{"$nulls":6},"铜","ND",0.5,"是"]
[{"$nulls":6},"pH值",6.68,"6-9","是"]
[11,"仲恺区","惠州市惠城区沥林屠宰场（惠州市仲恺高新区中心屠宰场）","废水排放口DW001","执行《肉类加工工业水污染物排放标准》（GB13457-92）表3畜类屠宰加工排放浓度三级标准","2025-03-10","动植物油","ND",60,"是"]
[{"$nulls":6},"氨氮",0.765,"-","是"]
[{"$nulls":6},"化学需氧量",40,500,"是"]
[{"$nulls":6},"大肠菌群数","1.1x105","-","是"]
[12,"仲恺区","惠州市惠城区沥林屠宰场（惠州市仲恺高新区中心屠宰场）","废水排放口DW001","执行《肉类加工工业水污染物排放标准》（GB13457-92）表3畜类屠宰加工排放浓度三级标准","2025-07-14","总氮",24.8,"-","-"]
[{"$nulls":6},"氨氮",23.2,"-","-"]
[{"$nulls":6},"化学需氧量",7,500,"是"]
[{"$nulls":6},"五日生化需氧量",4.8,300,"是"]
[{"$nulls":6},"大肠菌群数","2.8x102","-","-"]
[{"$nulls":6},"动植物油","ND",60,"是"]
[{"$nulls":6},"悬浮物",10,400,"是"]
[{"$nulls":6},"pH值",7.9,"6-8.5","是"]
[null,"仲恺区","惠州市惠城区沥林屠宰场（惠州市仲恺高新区中心屠宰场）","废水排放口DW001","执行《肉类加工工业水污染物排放标准》（GB13457-92）表3畜类屠宰加工排放浓度三级标准，《水污染物排放限值》（DB44/26-2001)第二时段三级标准和《惠州市第八污水处理厂设计进水水质标准》三者较严值","2025-09-18","总氮",7.83,"-","-"]
[{"$nulls":6},"氨氮",5.96,"-","-"]
[{"$nulls":6},"化学需氧量",11,500,"是"]
[{"$nulls":6},"悬浮物",10,400,"是"]
[{"$nulls":6},"pH值",7.5,"6-8.5","是"]
[null,"仲恺区","惠州市惠城区沥林屠宰场（惠州市仲恺高新区中心屠宰场）","废水排放口DW001","执行《肉类加工工业水污染物排放标准》（GB13457-92）表3畜类屠宰加工排放浓度三级标准，《水污染物排放限值》（DB44/26-2001)第二时段三级标准和《惠州市第八污水处理厂设计进水水质标准》三者较严值","2025-10-14","总氮",14.6,"-","是"]
[{"$nulls":6},"氨氮",0.197,"-","是"]
[{"$nulls":6},"化学需氧量",34,500,"是"]
[{"$nulls":6},"悬浮物",13,400,"是"]
[{"$nulls":6},"pH值",7.5,"6-8.5","是"]
[13,"仲恺区","惠州益伸电子有限公司","废水排放口DW003","执行《电镀水污染物排放标准》（DB44/1597-2015）表1珠三角标准及《水污染物排放限制》（DB44/26-2001）表4第二时段以及标准两者较严排放限制要求","2025-03-10","总氰化物",0.005,0.2,"是"]
[{"$nulls":6},"氨氮",1.58,10,"是"]
[{"$nulls":6},"化学需氧量",23,80,"是"]
[{"$nulls":6},"总磷",0.05,1,"是"]
[{"$nulls":6},"总氮",5.93,20,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":3},"废水排放口DW002",null,null,"总铬",0.04,0.5,"是"]
[{"$nulls":6},"六价铬","ND",0.1,"是"]
[{"$nulls":3},"废水排放口DW001",null,null,"总镍",0.12,0.5,"是"]
[14,"仲恺区","惠州益伸电子有限公司","废水排放口DW003","执行《电镀水污染物排放标准》DB44/1597-2015表1现有项目水污染物排放限值及单位产品基准排水量珠三角排放限值和《水污染排放限值》（DB44/26-2001）表4第二类污染物最高允许排放浓度（第二时段）一级标准中两者的较严值","2025-07-14","总氮",14.8,{"v":20,"d":"20.0"},"是"]
[{"$nulls":6},"氨氮",0.207,{"v":10,"d":"10.0"},"是"]
[{"$nulls":6},"总磷",0.05,1,"是"]
[{"$nulls":6},"化学需氧量",26,80,"是"]
[{"$nulls":6},"氰化物",0.005,0.2,"是"]
[{"$nulls":6},"氟化物",5.31,10,"是"]
[{"$nulls":6},"石油类","ND",2,"是"]
[{"$nulls":6},"悬浮物",9,30,"是"]
[{"$nulls":6},"铜","ND",0.5,"是"]
[{"$nulls":6},"锌","ND",{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"pH值",7.33,"6-9","是"]
[{"$nulls":3},"废水排放口DW002含铬废水排放口",null,null,"总铬","ND",0.5,"是"]
[{"$nulls":6},"六价铬","ND",0.1,"是"]
[{"$nulls":3},"废水排放口DW002含镍废水排放口",null,null,"镍","ND",0.5,"是"]
[15,"仲恺区","惠州市协昌智成电路有限公司","废水排放口DW001","执行广东省《水污染物排放限制》（DB/26-2001)表4第二类污染物最高允许排放浓度（第二时段一级标准），其余项目执行《电镀水污染物排放标准》（DB44/1597-2015)表1现有项目水污染物排放限值及单位产品基准排水量排放限值的珠三角标准","2025-03-21","总磷",0.01,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"化学需氧量",13,80,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":6},"总氮",2.94,20,"是"]
[null,"仲恺区","惠州市协昌智成电路有限公司","废水排放口DW001","执行广东省《水污染物排放限制》（DB/26-2001)表4第二类污染物最高允许排放浓度（第二时段一级标准），其余项目执行《电镀水污染物排放标准》（DB44/1597-2015)表1现有项目水污染物排放限值及单位产品基准排水量排放限值的珠三角标准","2025-09-17","总氮",3.65,20,"是"]
[{"$nulls":6},"氨氮",0.042,10,"是"]
[{"$nulls":6},"总磷",0.04,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"化学需氧量",22,80,"是"]
[{"$nulls":6},"氟化物",0.18,10,"是"]
[{"$nulls":6},"石油类","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"悬浮物","ND",30,"是"]
[{"$nulls":6},"总氰化物",0.007,0.2,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":6},"pH值",7.5,"6-9","是"]
[16,"仲恺区","惠州市肉联厂有限公司","废水排放口DW001","1、《肉类加工工业水污染物排放标准》（GB 13457-92）；\n2、广东省《水污染物排放限值》（DB 44/26-2001）；\n3、《淡水河、石马河流域水污染物排放标准》（DB 44/2050-2017）。","2025-03-21","动植物油","ND",10,"是"]
[{"$nulls":6},"总磷",0.02,0.5,"是"]
[{"$nulls":6},"氨氮",0.134,{"v":5,"d":"5.0"},"是"]
[{"$nulls":6},"化学需氧量",16,50,"是"]
[{"$nulls":6},"大肠菌群数",110,3000,"是"]
[17,"仲恺区","惠州市百瑞峰实业有限公司","废水排放口DW001","《地表水环境质量标准》（GB3838-2002）Ⅳ类水质标准","2025-03-27","阴离子表面活性剂","ND",{"v":5,"d":"5.0"},"是"]
[{"$nulls":6},"总磷",0.06,0.5,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"化学需氧量",15,80,"是"]
[null,"仲恺区","惠州市百瑞峰实业有限公司","废水排放口DW001","排放执行《纺织染整工业水污染物排放标准》（GB4287-2012)表2新建企业排放浓度限值及单位产品基准排水量间接排放限值与《水污染物排放限值》（DB44/26-201)中的第二时段三级排放标准两者较严值","2025-09-23","总磷",0.01,1.5,"是"]
[{"$nulls":6},"氨氮",0.032,20,"是"]
[{"$nulls":6},"化学需氧量",19,{"v":200,"d":"200.0"},"是"]
[{"$nulls":6},"悬浮物","ND",{"v":100,"d":"100.0"},"是"]
[{"$nulls":6},"五日生化需氧量",1.4,50,"是"]
[{"$nulls":6},"阴离子表面活性剂","ND","-","-"]
[{"$nulls":6},"pH值",7.8,"6-9","是"]
[18,"仲恺区","惠州市安利达五金制品有限公司","废水排放口DW001","石油类、氟化物（以F-计）、悬浮物、pH值、总磷（以P计）、化学需氧量、总氮（以N计）、总铝、总铁执行广东省《电镀水污染物排放标准》（DB44/1597-2015）中表1珠三角排放限值的标准；氨氮（NH3-N）执行广东省《水污染物排放限值》（DB44/26-2001）第二时段一级标准","2025-03-27","总磷",0.03,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"氨氮",0.058,10,"是"]
[{"$nulls":6},"化学需氧量",11,80,"是"]
[{"$nulls":6},"总铁","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"总氮",{"v":8.5,"d":"8.50"},20,"是"]
[null,"仲恺区","惠州市安利达五金制品有限公司","生产废水排放口DW001","执行《水污染物排放限值》（DB44/26-2001)中表4第二类污染物最高允许排放浓度第二时段一级标准和《电镀水污染物排放标准》DB44/1597-2015表1现有项目水污染物排放限值及单位产品基准排水量珠三角排放限值标准两者较严值。","2025-09-17","总氮",8.58,20,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"总磷",0.01,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"化学需氧量",16,80,"是"]
[{"$nulls":6},"氟化物",0.24,10,"是"]
[{"$nulls":6},"石油类","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"悬浮物","ND",30,"是"]
[{"$nulls":6},"总铁","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"pH值",{"v":7,"d":"7.0"},"6-9","是"]
[19,"仲恺区","惠州市仲恺高新区瑞泰五金加工厂","废水排放口DW002","石油类、氟化物（以F-计）、总氰化物、悬浮物、pH值、总磷（以P计）、化学需氧量、总氮（以N计）、总铝、总铁执行广东省《电镀水污染物排放标准》（DB44/1597-2015）中表1珠三角排放限值的标准；氨氮（NH3-N）执行广东省《水污染物排放限值》（DB44/26-2001）第二时段一级标准","2025-03-27","总氰化物","ND",0.2,"是"]
[{"$nulls":6},"氨氮",0.856,10,"是"]
[{"$nulls":6},"化学需氧量",26,80,"是"]
[{"$nulls":6},"总磷",0.14,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"总氮",4.57,20,"是"]
[{"$nulls":6},"总铁","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":3},"含镍废水排放口DW001","广东省地方标准《电镀水污染物排放标准》（DB 441597-2015）。",null,"总镍",0.06,0.5,"是"]
[20,"仲恺区","惠州建邦精密塑胶有限公司","废水排放口DW003","广东省地方标准《电镀水污染物排放标准》（DB 441597-2015）","2025-03-28","总磷",0.08,2,"是"]
[{"$nulls":6},"总氮",0.348,30,"是"]
[{"$nulls":6},"化学需氧量",18,160,"是"]
[{"$nulls":6},"总铜",0.08,1,"是"]
[{"$nulls":6},"总氮",1.18,40,"是"]
[null,"仲恺区","惠州建邦精密塑胶有限公司","废水排放口DW001","执行《电镀水污染物排放标准》(ZB44/1597-2015)表1现有项目水污染物排放限值及单位产品基准排水量的珠三角排放限值的200%，pH值执行100%。","2025-10-21","总磷",0.02,2,"是"]
[{"$nulls":6},"氨氮",0.052,30,"是"]
[{"$nulls":6},"化学需氧量",10,160,"是"]
[{"$nulls":6},"总氮",1.18,40,"是"]
[{"$nulls":6},"总铜",0.06,1,"是"]
[{"$nulls":6},"悬浮物","ND",60,"是"]
[{"$nulls":6},"石油类",0.13,4,"是"]
[{"$nulls":6},"氟化物",0.18,20,"是"]
[{"$nulls":6},"pH值",7.2,"6-9","是"]
[21,"仲恺区","惠州美锐电子科技有限公司","废水排放口DW001","《电镀污染物排放标准》（GB21900-2008）、《恶臭污染物排放标准》（GB14554-93）、《印刷行业挥发性有机化合物排放标准》（DB44/815-2010）、《大气污染物排放限值》（DB44/27-2001）","2025-03-31","总氰化物",0.038,0.2,"是"]
[{"$nulls":6},"氨氮",0.669,8,"是"]
[{"$nulls":6},"化学需氧量",22,50,"是"]
[{"$nulls":6},"总磷",0.03,0.5,"是"]
[{"$nulls":6},"总氮",8.21,15,"是"]
[{"$nulls":6},"总镍","ND",0.1,"是"]
[{"$nulls":6},"总铜","ND",0.3,"是"]
[{"$nulls":3},"含镍废水排放口DW003",null,null,"总镍","ND",0.1,"是"]
[22,"仲恺区","惠州美锐电子科技有限公司","DW001生产废水排放口","《电镀污染物排放标准》 DB 44/1597-2015表2新建项目水污染物排放限值及单位产品基准排水量珠三角排放限值和《电子工业水污染物排放标准》（GB39731-2020)表1水污染物排放限值的印制电路板排放标准两者的较严值。","2025-07-10","总氮",{"v":8.1,"d":"8.10"},15,"是"]
[{"$nulls":6},"氨氮",0.333,8,"是"]
[{"$nulls":6},"总磷",0.03,0.5,"是"]
[{"$nulls":6},"化学需氧量",19,50,"是"]
[{"$nulls":6},"氰化物","ND",0.2,"是"]
[{"$nulls":6},"氟化物",3.48,20,"是"]
[{"$nulls":6},"石油类",0.11,{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"悬浮物","ND",30,"是"]
[{"$nulls":6},"铜","ND",0.3,"是"]
[{"$nulls":6},"pH值",7.33,"6-9","是"]
[{"$nulls":3},"含镍废水排放口DW003",null,null,"镍","ND",0.1,"是"]
[23,"仲恺区","惠州中京电子科技有限公司","废水排放口DW001","1.《大气污染物排放限值》（DB44/27-2001）        2.《电镀污染物排放标准》（GB21900-2008)）","2025-03-31","总氰化物",0.025,0.4,"是"]
[{"$nulls":6},"氨氮",{"v":0.41,"d":"0.410"},30,"是"]
[{"$nulls":6},"化学需氧量",21,160,"是"]
[{"$nulls":6},"总磷",0.49,2,"是"]
[{"$nulls":6},"总氮",15.8,40,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[24,"仲恺区","信利（惠州）智能显示有限公司","废水排放口DW001","水污染物排放限值DB44/ 26—2001","2025-03-31","总氮",7.05,"-","-"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"化学需氧量",9,90,"是"]
[{"$nulls":6},"总磷",0.02,0.5,"是"]
[{"$nulls":6},"总锌","ND",{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[null,"仲恺区","信利（惠州）智能显示有限公司","废水排放口DW001","执行《水污染物排放限值》（DB44/26-2001）中表4第二类污染物最高允许排放浓度第二时段一级标准，《电子工业水污染物排放标准》GB39731-2020表1水污染物排放限值显示器件及光电子器件直接排放限值","2025-09-30","总氮",5.36,35,"是"]
[{"$nulls":6},"氨氮","ND",25,"是"]
[{"$nulls":6},"总磷",9,0.5,"是"]
[{"$nulls":6},"化学需氧量",1.67,90,"是"]
[{"$nulls":6},"氟化物","ND",10,"是"]
[{"$nulls":6},"石油类","ND",{"v":5,"d":"5.0"},"是"]
[{"$nulls":6},"悬浮物",0.005,60,"是"]
[{"$nulls":6},"总氰化物",0.005,0.3,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]
[{"$nulls":6},"pH值",7.1,"6-9","是"]
[25,"仲恺区","惠州市永兴达蓄电池有限公司","废水排放口DW001","《电池工业污染物排放标准》(GB30484-2013)表2中的直接排放限值","2025-03-31","总氮",2.14,15,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"化学需氧量",12,70,"是"]
[{"$nulls":6},"总磷",0.13,0.5,"是"]
[{"$nulls":6},"总铅","ND",15,"是"]
[null,"仲恺区","惠州市永兴达蓄电池有限公司","废水排放口DW001","《电池工业污染物排放标准》(GB30484-2013)表2中的直接排放限值","2025-09-17","总氮",1.38,15,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"总磷",0.02,0.5,"是"]
[{"$nulls":6},"化学需氧量",10,70,"是"]
[{"$nulls":6},"悬浮物","ND",50,"是"]
[{"$nulls":6},"总铅","ND",0.5,"是"]
[{"$nulls":6},"pH值",6.7,"6-9","是"]
[26,"仲恺区","泰和电路科技（惠州）有限公司","废水排放口DW002","广东省地方标准《电镀水污染物排放标准》（DB 441597-2015）","2025-03-31","总铜","ND",0.5,"是"]
[{"$nulls":6},"氨氮","ND",15,"是"]
[{"$nulls":6},"化学需氧量",7,80,"是"]
[{"$nulls":6},"总磷",0.07,0.1,"是"]
[{"$nulls":6},"总氮",1.42,20,"是"]
[{"$nulls":3},"含镍废水排放口DW001",null,null,"总镍","ND",0.5,"是"]
[27,"仲恺区","泰和电路科技（惠州）有限公司","DW002废水排放口","执行《电镀水污染物排放标准》DB44/1597-2015表1现有项目水污染物排放限值及单位产品基准排水量珠三角排放限值、广东省《水污物排放限值》DB44/26-2001表4第二类污染物最高允许排放浓度第二时段三级标准和《电子工业水污染物排放标准》（GB39731-2020)表1水污染物排放限值的印制电路板间接排放标准三者的较严值","2025-07-14","总氮",1.61,20,"是"]
[{"$nulls":6},"氨氮",0.056,15,"是"]
[{"$nulls":6},"总磷",0.05,{"v":1,"d":"1.0"},"是"]
[{"$nulls":6},"化学需氧量",7,80,"是"]
[{"$nulls":6},"氰化物",0.011,0.2,"是"]
[{"$nulls":6},"氟化物",0.22,10,"是"]
[{"$nulls":6},"石油类",0.09,{"v":2,"d":"2.0"},"是"]
[{"$nulls":6},"悬浮物","ND",30,"是"]
[{"$nulls":6},"铜","ND",0.5,"是"]
[{"$nulls":6},"pH值",7.23,"6-9","是"]
[{"$nulls":3},"DW001废水排放口",null,null,"镍","ND",0.5]
[28,"仲恺区","科罗贝电子（惠州）有限公司","废水排放口DW001","广东省地方标准《电镀水污染物排放标准》（DB 441597-2015）。","2025-04-09","总氮",2.89,20,"是"]
[{"$nulls":6},"氨氮","ND",10,"是"]
[{"$nulls":6},"化学需氧量",13,80,"是"]
[{"$nulls":6},"总磷",0.01,0.1,"是"]
[{"$nulls":6},"总铜","ND",0.5,"是"]