{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地下水"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地下水","index":0,"n_rows":13,"n_cols":24,"rows_kept":13,"merged":[[0,0,0,23],[1,6,1,23],[4,0,4,2],[5,0,5,2],[7,0,11,0]],"flags":["formulas_cached_only"]}
["附件5：                         惠州市2020年8月生活垃圾处理企业地下水监督性监测结果（2家）"]
[{"$nulls":6},"单位：毫克/升（除PH值无量纲）"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅"]
["博罗县垃圾填埋场","2020-07-30","项目西面山体路边井水",7.03,38.6,95,0.818,0.951,"0.03L","0.01L",0.0023,"0.05L","0.0003L",{"v":1,"d":"1.0"},0.785,0.026,0.32,0.074,"0.004L","0.00004L","0.0003L",0.00029,"0.004L",0.0301]
["评价",null,null,"达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","超2.01倍"]
["《地下水质量标准》（GB/T14848-2017）表1 Ⅲ类标准",null,null,"6.5—8.5",450,1000,250,250,0.3,{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},0.002,3,20,{"v":1,"d":"1.00"},{"v":0.5,"d":"0.50"},{"v":1,"d":"1.0"},0.05,0.001,0.01,0.005,0.05,0.01]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅"]
["惠阳区榄子垅垃圾综合处理项目生活垃圾填埋场","2020-07-21","1#地下水井取样点",7.03,34.9,327,1.124,2.992,0.15,"0.01L","0.0002L","0.05L","0.0003L",1.6,0.327,{"v":0.13,"d":"0.130"},0.57,0.342,"0.004L","0.00004L",0.0014,"0.00002L","0.004L","0.0002L"]
[null,"2020-07-21","2#地下水井取样点",7.01,470,165,21.79,326.7,"0.03L",0.09,"0.0002L","0.05L","0.0003L",3.6,0.327,0.268,0.22,0.929,"0.004L","0.00004L",0.0041,0.00033,"0.004L","0.0002L"]
[null,"2020-07-21","3#地下水井取样点",5.21,25.6,96,0.443,1.444,"0.03L","0.01L","0.0002L","0.05L","0.0003L",1.4,0.062,"0.003L",0.12,0.014,"0.004L","0.00004L",0.0015,"0.00002L","0.004L","0.0002L"]
[null,"2020-07-21","4#地下水井取样点",6.99,41.4,154,5.788,135.4,"0.03L",2.12,"0.0002L",0.38,"0.0003L",1.6,1.502,"0.003L",0.23,0.248,"0.004L","0.00004L",0.0017,1.3e-05,"0.004L","0.0002L"]
[null,"2020-07-21","6#地下水井取样点",{"v":6.6,"d":"6.60"},41.9,220,3.696,{"v":6.96,"d":"6.960"},"0.03L","0.01L",0.002,"0.05L","0.0003L",1.3,0.332,"0.003L",0.14,0.379,"0.004L","0.00004L",0.0017,"0.00002L","0.004L","0.0002L"]
["备注：惠阳区榄子垅垃圾综合处理项目生活垃圾填埋场地下水暂无评价依据。"]