{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地下水"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地下水","index":0,"n_rows":8,"n_cols":25,"rows_kept":8,"merged":[[0,0,0,24],[1,6,1,24],[3,0,6,0],[3,1,6,1],[7,0,7,2]],"flags":["formulas_cached_only"]}
["附件4：                         惠州市2020年10月生活垃圾处理企业地下水监督性监测结果（1家）"]
[{"$nulls":6},"单位：毫克/升（除PH值无量纲，粪大肠菌群为个/升外）"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅","粪大肠菌群"]
["惠东县垃圾填埋场","2020-09-11","废水站1号监测井",5.94,69.8,343,13.61,54.63,2.79,1.55,0.0014,"0.05L","0.0003L",2.4,1.677,0.006,0.27,0.067,"0.004L","0.00004L","0.0003L",0.00034,"0.004L","0.0002L","—"]
[null,null,"评价","偏低0.56个pH","达标","达标","达标","达标","超8.30倍","超14.50倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
[null,null,"项目正北方向3号扩散井",5.75,64.6,277,7.116,{"v":12.7,"d":"12.70"},3.61,0.83,0.0008,"0.05L","0.0003L",{"v":3,"d":"3.0"},0.227,"0.003L",0.38,"0.006L","0.004L","0.00004L","0.0003L",0.00039,"0.004L","0.0002L","—"]
[null,null,"评价","偏低0.75个pH","达标","达标","达标","达标","超11.03倍","超7.30倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
["《地下水质量标准》（GB/T14848-2017）Ⅲ类",null,null,"6.5—8.5",450,1000,250,250,0.3,0.1,{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},0.002,3,20,{"v":1,"d":"1.00"},{"v":0.5,"d":"0.50"},{"v":1,"d":"1.0"},0.05,0.001,0.01,0.005,0.05,0.01,"—"]