{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地下水"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地下水","index":0,"n_rows":6,"n_cols":25,"rows_kept":6,"merged":[[0,0,0,24],[1,6,1,24],[4,0,4,2],[5,0,5,2]],"flags":["formulas_cached_only"]}
["附件4：                         惠州市2020年11月生活垃圾处理企业地下水监督性监测结果（1家）"]
[{"$nulls":6},"单位：毫克/升（除PH值无量纲外）"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅","粪大肠菌群"]
["博罗县垃圾填埋场","2020-10-27","项目西面山体路边井水",6.92,42.2,801,0.786,0.632,0.0817,{"v":0.01,"d":"0.0100"},0.00127,0.0142,"0.0003L",0.8,0.391,"0.003L",0.17,0.039,"0.004L","0.00004L","0.0003L",0.00018,"0.004L",0.0239,"/"]
["评价",null,null,"达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","超1.39倍","—"]
["《地下水质量标准》（GB/T14848-2017）表1 Ⅲ类标准",null,null,"6.5—8.5",450,1000,250,250,0.3,{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},0.002,3,{"v":20,"d":"20.0"},{"v":1,"d":"1.00"},{"v":0.5,"d":"0.50"},{"v":1,"d":"1.0"},0.05,0.001,0.01,0.005,0.05,0.01,"—"]