{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地下水"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地下水","index":0,"n_rows":9,"n_cols":26,"rows_kept":9,"merged":[[0,0,0,24],[1,6,1,24],[3,0,6,0],[3,1,6,1],[3,25,5,25],[7,0,7,2]],"flags":["formulas_cached_only"]}
["附件5：                         惠州市2020年12月生活垃圾处理企业地下水监督性监测结果（2家）"]
[{"$nulls":6},"单位：毫克/升（除PH值无量纲，粪大肠菌群为个/升外）"]
["企业名称","监测日期","监测点位","pH值","总硬度","溶解性总固体","硫酸盐","氯化物","铁","锰","铜","锌","挥发酚","高锰酸盐指数","硝酸盐（硝酸盐氮）","亚硝酸（亚硝酸盐氮）","氨氮","氟化物","氰化物","汞","砷","镉","六价铬","铅","粪大肠菌群"]
["惠东县垃圾填埋场","2020-11-11","废水站1号监测井",5.85,93.1,223,8.716,38.42,0.0508,1.47,0.00011,0.0135,"0.0003L",{"v":1,"d":"1.0"},1.535,0.003,"0.04L",0.081,"0.004L","0.00004L","0.0003L",0.00027,"0.004L","0.00009L","20L","12月公布"]
[null,null,"评价","偏酸0.65个pH","达标","达标","达标","达标","达标","超13.70倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
[null,null,"项目正北方向3号扩散井",5.74,28.6,280,0.399,{"v":17.9,"d":"17.90"},0.00161,0.359,0.00047,0.0274,"0.0003L",4.9,0.091,"0.003L","0.04L",{"v":0.05,"d":"0.050"},"0.004L","0.00004L","0.0003L",0.00028,"0.004L","0.00009L","20L"]
[null,null,"评价","偏酸0.76个pH","达标","达标","达标","达标","达标","超2.59倍","达标","达标","达标","超0.63倍","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","—"]
["《地下水质量标准》（GB/T14848-2017）Ⅲ类",null,null,"6.5—8.5",450,1000,250,250,0.3,0.1,{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},0.002,3,20,{"v":1,"d":"1.00"},{"v":0.5,"d":"0.50"},{"v":1,"d":"1.0"},0.05,0.001,0.01,0.005,0.05,0.01,"—"]
["龙门县垃圾填埋场\n（龙门县甘香垃圾场）","2020-11-16","垃圾场地下水监测井",6.35,11.7,48,1.182,6.651,5.26,0.0909,0.00028,0.0874,"0.0003L",4.5,"0.016L","0.003L",0.32,0.055,"0.004L","0.00004L","0.0003L","0.00005L","0.004L","0.00009L",90,"12月公布"]